ThingSpeak Communication Library Enables an Arduino, ESP8266, or Particle to write or read data to or from ThingSpeak™ |

- Main Page
- Data Structures

- Data Structures
- Data Fields

- All
- Functions

- begin() : ThingSpeakClass
- getLastReadStatus() : ThingSpeakClass
- readFloatField() : ThingSpeakClass
- readIntField() : ThingSpeakClass
- readLongField() : ThingSpeakClass
- readRaw() : ThingSpeakClass
- readStringField() : ThingSpeakClass
- setElevation() : ThingSpeakClass
- setField() : ThingSpeakClass
- setLatitude() : ThingSpeakClass
- setLongitude() : ThingSpeakClass
- writeField() : ThingSpeakClass
- writeFields() : ThingSpeakClass
- writeRaw() : ThingSpeakClass